8.15. 29West
Prev | Chapter 8. Statistics | Next

## 8.15. 29West

The 29West technology now refers to Ultra-Low Latency Messaging (ULLM) technology. It allows sending and receiving a high number of messages per second with microsecond delivery times for zero-latency data delivery.

The Statistics → 29West shows:

The `Topics` submenu shows counters for: | Advertisement by Topic Advertisement by Source Advertisement by Transport Queries by Topic Queries by Receiver Wildcard Queries by Pattern Wildcard Queries by Receiver
The `Queues` submenu shows counters for: | Advertisement by Queue Advertisement by Source Queries by Queue Queries by Receiver
The `UIM` submenu shows `Streams`: | Each stream is provided by Endpoints, Messages, Bytes, and the First and Last Frame statistics.
The `LBT-RM` submenu | The LBT-RM Transport Statistics window shows the Sources and Receivers sequence numbers for transport and other data.
The `LBT-RU` submenu | The LBT-Ru Transport Statistics window shows the Sources and Receivers sequence numbers for transport and other data.

Prev | Up | Next
8.14. ONC-RPC Programs | Home | 8.16. ANCP