3.19. The “Packet Details” Pane
Prev | Chapter 3. User Interface | Next

## 3.19. The “Packet Details” Pane

The packet details pane shows the current packet (selected in the “Packet List” pane) in a more detailed form.

Figure 3.17. The “Packet Details” pane

This pane shows the protocols and protocol fields of the packet selected in the “Packet List” pane. The protocol summary lines (subtree labels) and fields of the packet are shown in a tree which can be expanded and collapsed.

There is a context menu (right mouse click) available. See details in Figure 6.5, “Pop-up menu of the “Packet Details” pane”.

Some protocol fields have special meanings.

- Generated fields. Wireshark itself will generate additional protocol information which isn’t present in the captured data. This information is enclosed in square brackets (“[” and “]”). Generated information includes response times, TCP analysis, IP geolocation information, and checksum validation.
- Links. If Wireshark detects a relationship to another packet in the capture file it will generate a link to that packet. Links are underlined and displayed in blue. If you double-click on a link, Wireshark will jump to the corresponding packet.

Prev | Up | Next
3.18. The “Packet List” Pane | Home | 3.20. The “Packet Bytes” Pane